智能测试杯操作说明

Thank you for purchasing the intellectual testing cup of our company, the main functions of this product are as follows:

Material: both the inside and outside of this cup are vacuum of food grade 304 stainless steel. The cup lid, which is made of environment-friendly ABS+ soft silica gel material, is made up of the following electronic function parts: Hi-fi loudspeaker with inner magnetic rubber edge, environment-friendly PCB circuit board, digital display, polymer lithium battery and etc..

使用时要小心:因为杯盖是电子零件，不防水。请放入水中清洗或消毒。清洁时，请用湿毛巾擦拭。为防止内部零件脱落，影响正常使用，请不要从高处抛掷或掉落。高温可能会导致电池爆炸，请不要把它放在火里。

Please read the following detailed instruction:

使用前，请先清洗(用沸水注满杯子，拧紧盖子，然后摇动)。由于盖子在日常使用中是防水的，它不能经受浸泡和淋湿，请防止盖子落入水中。请参考图1中杯盖的介绍。要启动，请长按电源键。

当语音提示低电量和电池图标闪烁时，请充电。参见图3，打开盖子的USB盖，插入充电电缆，并将电缆的另一侧插入充电头或电脑的USB插座。充电电压超过5V1A会烧毁内部线路。正常充电时，图2中的电池图标会闪烁。停止闪烁表示电池已充满电。如果充电超过10分钟后没有上述反应，一定有问题。你可以尝试通过更换充电电缆(充电电缆与安卓手机的充电电缆相同)或更换充电头来解决这个问题。如果两种方法都不起作用，电池或电线一定有问题。此时您可以要求售后服务。